AVENIR CASTLE – LARGE TOWER Catalogue number: 72502

It shall apply from: 2024-06-27

Max. free fall height:	0,98 m
Product Dimensions: (length x width x height)	3,49 x 0,77 x 2,63 m
Impact area: (length x width)	6,27 x 3,71 m

Impact area dimensions
3,71 m	0,77 m	Permissible impact attenuating surface
Turf Bark – grain size 20 do 80 mm, min. depth 200 mm + 100mm (for displacement) Woodchip – grain size 5 do 30 mm, min. depth 200mm + 100mm (for displacement) Sand – grain size 0,2 do 2 mm, min. depth 200mm + 100mm (for displacement) Synthetic surfaces in accordance whit tested HIC (EN 1177)
The impact attenuating surfacing shall be installed on the whole of impact area. A loose surface should be made so that its thickness is 100 mm greater than the minimum value given above.
3,49 m
6,27 m

Technical description
Construction made of steel pipes Ø48,3x2,9mm, Surface elements made of 8mm thick HPL boards decorated with colourful prints resistant to UV radiation Floor platforms made of anti-slip, waterproof plywood, 21mm thick, Slide made of stainless steel and milled HPL board 10mm thick The steel structure is hot-dip galvanized and powder-coated, The set includes foundations made of concrete of class C25/30.

List of components
Bottom construction with counter x 1pc Tower W4-950-ZD4 x 1pc Climbing entrance H950 B x 1pc Stairs H950 x1szt Side panel B1 H950 x 1pc Side panel A2 Dragon H950 x 1pc Dragon slide H950 x 1pc Top of the tower D4 x 1pc

Product visualization